**ASSIGNMENT -3**

**CHARULATHA N B**

**710719106016**

**PYTHON CODE FOR BLINKING LED**

import RPi.GPIO as GPIO # Import Raspberry Pi GPIO library

from time import sleep # Import the sleep function from the time module

GPIO.setwarnings(False) # Ignore warning for now

GPIO.setmode(GPIO.BOARD) # use physical pin numbering

GPIO.setup(8, GPIO.OUT, initial=GPIO.LOW) # Set pin 8 to be an output pin and set initial value to low (off)

while True: # Run forever

GPIO.output(8, GPIO.HIGH) #Turn on

Sleep (1) #sleep for 1 second

GPIO.output(8, GPIO.LOW) #Turn off

Sleep (1) #sleep for 1 second

**PYTHON CODE FOR TRAFFIC LIGHT**

import RPi.GPIO as GPIO

import time

import signal

import sys

# Setup

GPIO.setmode(GPIO.BCM)

GPIO.setup(9, GPIO.OUT)

GPIO.setup(10, GPIO.OUT)

GPIO.setup(11, GPIO.OUT)

# Turn off all lights when user ends demo

def allLightsOff(signal, frame):

GPIO.output(9, False)

GPIO.output(10, False)

GPIO.output(11, False)

GPIO.cleanup()

sys.exit(0)

signal.signal(signal.SIGINT, allLightsOff)

# Loop forever

while True:

# Red

GPIO.output(9, True)

time.sleep(3)

# Red and amber

GPIO.output(10, True)

time.sleep(1)

# Green

GPIO.output(9, False)

GPIO.output(10, False)

GPIO.output(11, True)

time.sleep(5)

# Amber

GPIO.output(11, False)

GPIO.output(10, True)

time.sleep(2)

# Amber off (red comes on at top of loop)

GPIO.output(10, False)